Livre interactif pour enfant avec capteur de pression

Porteur(s) du projet : Vincent Rosier (DSAA 1), Damien MUTI (Prof. de Numérique)

Date : 03/2021

Contexte : Micro-projet de cours

Fichiers :

Liens : https://www.instructables.com/Interfacing-Force-Sensitive-Resistor-to-Arduino/

Capteurs/Actionneurs :

Carte Arduino Uno /Seeduino

Capteur de pression (force)

Intentions : explication du projet et objectifs

Dans le cadre d'une édition jeunesse, l'objectif est de réaliser un livre interactif afin de susciter la manipulation et de rendre acteur l'enfant. À l'aide d'un capteur de pression dissimulé dans une page, des sons et/ou formes seront générés sur Processing lorsque l'enfant appuieras sur celui-ci. Ces sons et/ou formes pourront varier en intensité (sonore / taille de la forme / couleur) ou bien se multiplier en fonction de la force transmise sur le capteur.

Plans et schémas de fonctionnement

. Faire varier l'intensité d'une led ou d'une forme sur processing

Programmes

ARDUINO

. faire varier l'intensité d'une led

int fsrAnalogPin = 0; / FSR connecté a A0

int LEDpin = 11; / D11 pate de la LED

int fsrReading; / lecture du capteur FSR

int LEDbrightness;

void setup() {

// déclare ledPin comme une sortie numérique
Serial.begin(9600); // ouverture du port série
pinMode(LEDpin, OUTPUT);

}

void loop() {

fsrReading = analogRead(fsrAnalogPin);
Serial.print("Analog reading = ");
Serial.println(fsrReading);

/ Degrès d'intentsité de la luminosité de la LED

LEDbrightness = map(fsrReading, 0, 1023, 0, 255);
// La LED devient plus brillante lorsqu'on appuie plus fort
analogWrite(LEDpin, LEDbrightness);

delay(100); }

. Variation forme graphique

int firstSensor = 0; / first analog sensor

int inByte = 0; / incoming serial byte

void setup() {

// start serial port at 9600 bps:
Serial.begin(9600);
while (!Serial) {
; // wait for serial port to connect. Needed for native USB port only
}

pinMode(2, INPUT); // digital sensor is on digital pin 2
establishContact(); // send a byte to establish contact until receiver responds

}

void loop() {

// if we get a valid byte, read analog ins:
if (Serial.available() > 0) {
// get incoming byte:
inByte = Serial.read();
// read first analog input, divide by 4 to make the range 0-255:
firstSensor = analogRead(A0)/4;
// send sensor values:
Serial.write(firstSensor);
delay(10); // patienter 10ms (à voir...)
}

}

void establishContact() {

while (Serial.available() <= 0) {
Serial.print('A'); // send a capital A
delay(300);
}

}

PROCESSING

. Variation forme graphique

import processing.serial.*;

int bgcolor[] = {255, 255, 255}; / Background color

int fgcolor =255; / Fill color

int xpos, ypos; / Starting position of the ball

int rayon = 20;

Serial myPort; / The serial port

int serialInArray; / Where we'll put what we receive

int serialCount = 0; / A count of how many bytes we receive

boolean firstContact = false; / Whether we've heard from the microcontroller

void setup() {

size(500, 500); // Stage size
noStroke(); // No border on the next thing drawn

// Set the starting position of the ball (middle of the stage)
xpos = width/2;
ypos = height/2;

// Print a list of the serial ports, for debugging purposes:
printArray(Serial.list());

// I know that the first port in the serial list on my mac
// is always my FTDI adaptor, so I open Serial.list()[0].
// On Windows machines, this generally opens COM1.
// Open whatever port is the one you're using.
String portName = Serial.list()[0];
myPort = new Serial(this, portName, 9600);

// espace HSB des couleurs
colorMode(HSB);

}

void draw() {

rectMode(CENTER);
background(0);
fill (255, 255, 200);
circle(xpos,ypos,rayon);

}

void serialEvent(Serial myPort) {

// read a byte from the serial port:
int inByte = myPort.read();////////////////////////////////////////
// if this is the first byte received, and it's an A,
// clear the serial buffer and note that you've
// had first contact from the microcontroller.
// Otherwise, add the incoming byte to the array:
if (firstContact == false) {
if (inByte == 'A') {
myPort.clear(); // clear the serial port buffer
firstContact = true; // you've had first contact from the microcontroller
myPort.write('A'); // ask for more
}
} else {
rayon= (int)map(inByte, 0,255,20,400);
// print the values (for debugging purposes only):
println("valeur lue sur le port Série = " + rayon);

// Send a capital A to request new sensor readings:
myPort.write('A');
}

}

Réalisation de la maquette

. Vidéos

- Faire varier l'intensité d'une LED : https://youtu.be/Ll94pqV1qZw - Faire varier une forme graphique sur Processing : https://youtu.be/0GPNYONl8aM